1. Create Method from Reference Out of BSC Device. Select CloseDevice.
2. Create Method from Device output of BSC Device. Select GetChannel.
3. Under Function Palette/Programming/Application Control select “To More Generic Class” and wire reference of this to BSC GetChannel output.
4. From Target Class output of the To More Generic Class (found on top), create a constant. Right click on constant, Select .NET class, and Browse. Follow to GenericMotorCLI.AdvancedMotor.GenericAdvancedMotorCLI.
5. From Generic Class Reference output, Create Method. You should have the full list of methods here.

